# 常量字段值

## 目录

- com.ad.*

## com.ad.*

- com.ad.comm.CommStatus
  限定符和类型 | 常量字段 | 值
  --- | --- | ---
  `public static final int` | `CONNECT_EXCEPT` | `4`
  `public static final int` | `CONNECT_FAIL` | `3`
  `public static final int` | `CONNECT_OK` | `0`
  `public static final int` | `CONNECT_TIMEOUT` | `2`
  `public static final int` | `CONNECTING` | `1`
  `public static final int` | `DISCONNECT_EXCEPT` | `14`
  `public static final int` | `DISCONNECT_FAIL` | `13`
  `public static final int` | `DISCONNECT_OK` | `10`
  `public static final int` | `DISCONNECT_TIMEOUT` | `12`
  `public static final int` | `DISCONNECTING` | `11`
  `public static final int` | `OTHER` | `1001`
  `public static final int` | `RECEIVE_EXCEPT` | `34`
  `public static final int` | `RECEIVE_FAIL` | `33`
  `public static final int` | `RECEIVE_OK` | `30`
  `public static final int` | `RECEIVE_TIMEOUT` | `32`
  `public static final int` | `RECEIVEING` | `31`
  `public static final int` | `SEND_EXCEPT` | `24`
  `public static final int` | `SEND_FAIL` | `23`
  `public static final int` | `SEND_OK` | `20`
  `public static final int` | `SEND_TIMEOUT` | `22`
  `public static final int` | `SENDING` | `21`

- com.ad.comm.CommType
  限定符和类型 | 常量字段 | 值
  --- | --- | ---
  `public static final int` | `BLE` | `4`
  `public static final int` | `BLUETOOTH` | `3`
  `public static final int` | `NET` | `1`
  `public static final int` | `SERIAL` | `0`
  `public static final int` | `USB` | `2`

- com.ad.comm.usb.ADConstants
  限定符和类型 | 常量字段 | 值
  --- | --- | ---
  `public static final int` | `USB_CLASS_APP_SPEC` | `254`
  `public static final int` | `USB_CLASS_AUDIO` | `1`
  `public static final int` | `USB_CLASS_CDC_DATA` | `10`
  `public static final int` | `USB_CLASS_COMM` | `2`
  `public static final int` | `USB_CLASS_CONTENT_SEC` | `13`
  `public static final int` | `USB_CLASS_CSCID` | `11`
  `public static final int` | `USB_CLASS_HID` | `3`
  `public static final int` | `USB_CLASS_HUB` | `9`
  `public static final int` | `USB_CLASS_MASS_STORAGE` | `8`
  `public static final int` | `USB_CLASS_MISC` | `239`
  `public static final int` | `USB_CLASS_PER_INTERFACE` | `0`
  `public static final int` | `USB_CLASS_PHYSICA` | `5`
  `public static final int` | `USB_CLASS_PRINTER` | `7`
  `public static final int` | `USB_CLASS_STILL_IMAGE` | `6`
  `public static final int` | `USB_CLASS_VENDOR_SPEC` | `255`
  `public static final int` | `USB_CLASS_VIDEO` | `14`
  `public static final int` | `USB_CLASS_WIRELESS_CONTROLLER` | `224`
  `public static final byte` | `USB_DIR_IN` | `-128`
  `public static final byte` | `USB_DIR_OUT` | `0`
  `public static final byte` | `USB_ENDPOINT_DIR_MASK` | `-128`
  `public static final byte` | `USB_ENDPOINT_NUMBER_MASK` | `15`
  `public static final byte` | `USB_ENDPOINT_XFER_BULK` | `2`
  `public static final byte` | `USB_ENDPOINT_XFER_CONTROL` | `0`
  `public static final byte` | `USB_ENDPOINT_XFER_INT` | `3`
  `public static final byte` | `USB_ENDPOINT_XFER_ISOC` | `1`
  `public static final byte` | `USB_ENDPOINT_XFERTYPE_MASK` | `3`
  `public static final int` | `USB_INTERFACE_SUBCLASS_BOOT` | `1`
  `public static final int` | `USB_SUBCLASS_VENDOR_SPEC` | `255`
  `public static final byte` | `USB_TYPE_CLASS` | `32`
  `public static final byte` | `USB_TYPE_MASK` | `96`
  `public static final byte` | `USB_TYPE_RESERVED` | `96`
  `public static final byte` | `USB_TYPE_STANDARD` | `0`
  `public static final byte` | `USB_TYPE_VENDOR` | `64`

- com.ad.rfid.DeviceMode
  限定符和类型 | 常量字段 | 值
  --- | --- | ---
  `public static final int` | `ACTIVE` | `0`
  `public static final int` | `IMPINJ` | `3`
  `public static final int` | `OTHER` | `8`
  `public static final int` | `PASSIVE` | `1`
  `public static final int` | `PHYCHIPS` | `2`

- com.ad.rfid.passive.PassiveRcp
  限定符和类型 | 常量字段 | 值
  --- | --- | ---
  `public static final byte` | `INDEX_ADDRESS` | `1`
  `public static final byte` | `INDEX_CODE` | `3`
  `public static final byte` | `INDEX_LENGTH` | `5`
  `public static final byte` | `INDEX_PAYLOAD` | `6`
  `public static final byte` | `INDEX_PREAMBLE` | `0`
  `public static final byte` | `INDEX_TYPE` | `4`
  `public static final byte` | `LEN_CHECKSUM` | `1`
  `public static final byte` | `LEN_ENDMARK` | `0`
  `public static final byte` | `LEN_PROTOCOL_MIN` | `7`
  `public static final byte` | `PREAMBLE` | `124`
  `public static final byte` | `PREAMBLE_UP` | `-52`
  `public static final byte` | `RCP_CMD_CANBUS` | `-72`
  `public static final byte` | `RCP_CMD_EPC_APPOINT` | `34`
  `public static final byte` | `RCP_CMD_EPC_IDEN` | `16`
  `public static final byte` | `RCP_CMD_EPC_KILL` | `22`
  `public static final byte` | `RCP_CMD_EPC_LOCK` | `20`
  `public static final byte` | `RCP_CMD_EPC_MULT` | `17`
  `public static final byte` | `RCP_CMD_EPC_RW` | `18`
  `public static final byte` | `RCP_CMD_EPC_UNLOCK` | `21`
  `public static final byte` | `RCP_CMD_INFO` | `-126`
  `public static final byte` | `RCP_CMD_INITSYRIS` | `-115`
  `public static final byte` | `RCP_CMD_ISO6B_IDEN` | `1`
  `public static final byte` | `RCP_CMD_ISO6B_KILL` | `6`
  `public static final byte` | `RCP_CMD_ISO6B_LOCK` | `4`
  `public static final byte` | `RCP_CMD_ISO6B_RW` | `2`
  `public static final byte` | `RCP_CMD_ISO6B_UNLOCK` | `5`
  `public static final byte` | `RCP_CMD_OUTCARD` | `49`
  `public static final byte` | `RCP_CMD_PARA` | `-127`
  `public static final byte` | `RCP_CMD_REMOTE` | `-69`
  `public static final byte` | `RCP_CMD_SECRET` | `48`
  `public static final byte` | `RCP_CMD_SOFTRESET` | `-113`
  `public static final byte` | `RCP_CMD_SYRIS` | `-70`
  `public static final byte` | `RCP_CMD_TCPIP` | `-71`
  `public static final byte` | `RCP_CMD_TIME` | `-125`
  `public static final byte` | `RCP_CMD_USBPARA` | `-67`
  `public static final byte` | `RCP_CMD_USBPOWER` | `-68`
  `public static final byte` | `RCP_CMD_WIFI_AP` | `-22`
  `public static final byte` | `RCP_CMD_WIFI_DOWNLOAD` | `-25`
  `public static final byte` | `RCP_CMD_WIFI_PUB` | `-24`
  `public static final byte` | `RCP_CMD_WIFI_STA` | `-23`
  `public static final byte` | `RCP_MSG_GET` | `50`
  `public static final byte` | `RCP_MSG_SENIOR_GET` | `34`
  `public static final byte` | `RCP_MSG_SENIOR_SET` | `33`
  `public static final byte` | `RCP_MSG_SET` | `49`

- com.ad.rfid.phychips.PhychipsRcp
  限定符和类型 | 常量字段 | 值
  --- | --- | ---
  `public static final byte` | `ENDMARK` | `126`
  `public static final byte` | `HEADER_CMD` | `0`
  `public static final byte` | `INDEX_ADDRESS` | `1`
  `public static final byte` | `INDEX_CODE` | `3`
  `public static final byte` | `INDEX_LENGTH` | `5`
  `public static final byte` | `INDEX_PAYLOAD` | `6`
  `public static final byte` | `INDEX_PREAMBLE` | `0`
  `public static final byte` | `INDEX_TYPE` | `4`
  `public static final byte` | `LEN_CHECKSUM` | `1`
  `public static final byte` | `LEN_ENDMARK` | `0`
  `public static final byte` | `LEN_PROTOCOL_MIN` | `7`
  `public static final byte` | `PREAMBLE` | `124`
  `public static final byte` | `PREAMBLE_UP` | `-52`
  `public static final byte` | `RCP_CMD_AD_ADDR` | `-30`
  `public static final byte` | `RCP_CMD_AD_CUSTOM` | `-31`
  `public static final byte` | `RCP_CMD_AD_DATA` | `-27`
  `public static final byte` | `RCP_CMD_AD_IOOUT` | `-28`
  `public static final byte` | `RCP_CMD_AD_OUTCARD` | `-29`
  `public static final byte` | `RCP_CMD_AD_REMOTE` | `-69`
  `public static final byte` | `RCP_CMD_AD_UART` | `-26`
  `public static final byte` | `RCP_CMD_BLOCKERASE_C_DT` | `72`
  `public static final byte` | `RCP_CMD_BLOCKWRITE_C_DT` | `71`
  `public static final byte` | `RCP_CMD_CTL_RD_CON` | `2`
  `public static final byte` | `RCP_CMD_CTL_RD_PWR` | `1`
  `public static final byte` | `RCP_CMD_CTL_RESET` | `8`
  `public static final byte` | `RCP_CMD_GET_ANTICOL_MODE` | `52`
  `public static final byte` | `RCP_CMD_GET_AT_RD_PARM` | `15`
  `public static final byte` | `RCP_CMD_GET_C_QRY_PARM` | `13`
  `public static final byte` | `RCP_CMD_GET_C_SEL_PARM` | `11`
  `public static final byte` | `RCP_CMD_GET_CH` | `17`
  `public static final byte` | `RCP_CMD_GET_FH_LBT` | `19`
  `public static final byte` | `RCP_CMD_GET_HOPPING_TBL` | `48`
  `public static final byte` | `RCP_CMD_GET_LAST_RST` | `-95`
  `public static final byte` | `RCP_CMD_GET_MODEM_REG` | `-88`
  `public static final byte` | `RCP_CMD_GET_MODEM92_REG` | `-114`
  `public static final byte` | `RCP_CMD_GET_MODULATION` | `50`
  `public static final byte` | `RCP_CMD_GET_RD_INF` | `3`
  `public static final byte` | `RCP_CMD_GET_REGION` | `6`
  `public static final byte` | `RCP_CMD_GET_RF_REG` | `-87`
  `public static final byte` | `RCP_CMD_GET_RSSI` | `-59`
  `public static final byte` | `RCP_CMD_GET_RX_GAIN` | `-64`
  `public static final byte` | `RCP_CMD_GET_SIG_ST` | `4`
  `public static final byte` | `RCP_CMD_GET_TX_MODULE_PWR` | `-77`
  `public static final byte` | `RCP_CMD_GET_TX_PWR` | `21`
  `public static final byte` | `RCP_CMD_INFO` | `-126`
  `public static final byte` | `RCP_CMD_INVALID` | `0`
  `public static final byte` | `RCP_CMD_KILL_RECOM_C` | `101`
  `public static final byte` | `RCP_CMD_LOCK_C` | `-126`
  `public static final byte` | `RCP_CMD_MODEM_SINGLEREAD` | `-30`
  `public static final byte` | `RCP_CMD_NACK` | `-1`
  `public static final byte` | `RCP_CMD_NXP_CALIBRATE` | `86`
  `public static final byte` | `RCP_CMD_NXP_CHANGE_EAS` | `84`
  `public static final byte` | `RCP_CMD_NXP_EAS_ALARM` | `85`
  `public static final byte` | `RCP_CMD_NXP_READPROTECT` | `82`
  `public static final byte` | `RCP_CMD_NXP_RESET_READPROTECT` | `83`
  `public static final byte` | `RCP_CMD_PERMALOCK_C` | `-125`
  `public static final byte` | `RCP_CMD_READ_C_DT` | `41`
  `public static final byte` | `RCP_CMD_READ_C_ENTIRE` | `38`
  `public static final byte` | `RCP_CMD_READ_C_UII` | `34`
  `public static final byte` | `RCP_CMD_READ_C_USR_DT` | `36`
  `public static final byte` | `RCP_CMD_SCAN_RSSI` | `-58`
  `public static final byte` | `RCP_CMD_SECRET` | `48`
  `public static final byte` | `RCP_CMD_SET_ANT_PATH` | `-76`
  `public static final byte` | `RCP_CMD_SET_ANTICOL_MODE` | `53`
  `public static final byte` | `RCP_CMD_SET_AT_RD_PARM` | `16`
  `public static final byte` | `RCP_CMD_SET_C_QRY_PARM` | `14`
  `public static final byte` | `RCP_CMD_SET_C_SEL_PARM` | `12`
  `public static final byte` | `RCP_CMD_SET_CH` | `18`
  `public static final byte` | `RCP_CMD_SET_CW` | `23`
  `public static final byte` | `RCP_CMD_SET_DELI` | `-66`
  `public static final byte` | `RCP_CMD_SET_DOWNLOAD` | `-79`
  `public static final byte` | `RCP_CMD_SET_DUMP` | `-77`
  `public static final byte` | `RCP_CMD_SET_FH_LBT` | `20`
  `public static final byte` | `RCP_CMD_SET_HOPPING_TBL` | `49`
  `public static final byte` | `RCP_CMD_SET_INV_MODE` | `18`
  `public static final byte` | `RCP_CMD_SET_LED` | `-18`
  `public static final byte` | `RCP_CMD_SET_MOD_BLF` | `-65`
  `public static final byte` | `RCP_CMD_SET_MOD_DEPTH` | `-68`
  `public static final byte` | `RCP_CMD_SET_MODEM_REG` | `-90`
  `public static final byte` | `RCP_CMD_SET_MODEM92_REG` | `-115`
  `public static final byte` | `RCP_CMD_SET_MODULATION` | `51`
  `public static final byte` | `RCP_CMD_SET_MODULE_TABLE` | `-67`
  `public static final byte` | `RCP_CMD_SET_REGION` | `7`
  `public static final byte` | `RCP_CMD_SET_RF_REG` | `-89`
  `public static final byte` | `RCP_CMD_SET_RX_GAIN` | `-63`
  `public static final byte` | `RCP_CMD_SET_SIG_ST` | `5`
  `public static final byte` | `RCP_CMD_SET_TX_MODULE_PWR` | `-78`
  `public static final byte` | `RCP_CMD_SET_TX_OFFSET` | `-72`
  `public static final byte` | `RCP_CMD_SET_TX_PWR` | `22`
  `public static final byte` | `RCP_CMD_SET_TX_PWR_CL` | `-70`
  `public static final byte` | `RCP_CMD_STOP_AUTO_READ` | `40`
  `public static final byte` | `RCP_CMD_STOP_AUTO_READ_EX` | `55`
  `public static final byte` | `RCP_CMD_STOP_RX_TEST` | `-91`
  `public static final byte` | `RCP_CMD_STOP_TEST_MOD` | `-93`
  `public static final byte` | `RCP_CMD_STRT_AUTO_READ` | `39`
  `public static final byte` | `RCP_CMD_STRT_AUTO_READ_EX` | `54`
  `public static final byte` | `RCP_CMD_STRT_RX_TEST` | `-92`
  `public static final byte` | `RCP_CMD_STRT_TEST_MOD` | `-94`
  `public static final byte` | `RCP_CMD_VENDOR_SPECIFIC_02` | `19`
  `public static final byte` | `RCP_CMD_VENDOR_SPECIFIC_03` | `20`
  `public static final byte` | `RCP_CMD_VENDOR_SPECIFIC_04` | `21`
  `public static final byte` | `RCP_CMD_VENDOR_SPECIFIC_05` | `22`
  `public static final byte` | `RCP_CMD_WIFI_AP` | `-22`
  `public static final byte` | `RCP_CMD_WIFI_DOWNLOAD` | `-25`
  `public static final byte` | `RCP_CMD_WIFI_PUB` | `-24`
  `public static final byte` | `RCP_CMD_WIFI_STA` | `-23`
  `public static final byte` | `RCP_CMD_WRIT_C_DT` | `70`
  `public static final byte` | `RCP_ERASE_FLASH` | `-45`
  `public static final byte` | `RCP_GET_MSG_BUF_CNT` | `-40`
  `public static final byte` | `RCP_GET_REGISTRY_ITEM` | `-44`
  `public static final byte` | `RCP_GET_TEMPERATURE` | `-73`
  `public static final byte` | `RCP_MSG_AUTO` | `5`
  `public static final byte` | `RCP_MSG_CAP` | `4`
  `public static final byte` | `RCP_MSG_CMD` | `0`
  `public static final byte` | `RCP_MSG_GET` | `50`
  `public static final byte` | `RCP_MSG_NOTI` | `2`
  `public static final byte` | `RCP_MSG_RSP` | `1`
  `public static final byte` | `RCP_MSG_SET` | `49`
  `public static final byte` | `RCP_MSG_TEST` | `3`
  `public static final byte` | `RCP_SET_INT_PARAM` | `-48`
  `public static final byte` | `RCP_SET_LT` | `-38`
  `public static final byte` | `RCP_SET_REGISTRY_ITEM` | `-43`
  `public static final byte` | `RCP_TEST_EPC_QRYACK` | `34`
  `public static final byte` | `RCP_TEST_EPC_QRYQRYREP` | `35`
  `public static final byte` | `RCP_TEST_EPC_SEL` | `32`
  `public static final byte` | `RCP_TEST_EPC_SELQRY` | `33`
  `public static final byte` | `RCP_TEST_MODEM_RX` | `1`
  `public static final byte` | `RCP_TEST_MODEM_SEL_REP_E` | `3`
  `public static final byte` | `RCP_TEST_PKT_CAP_ACK` | `17`
  `public static final byte` | `RCP_TEST_PKT_CAP_UII` | `18`
  `public static final byte` | `RCP_TEST_PKT_CAPTURE` | `16`
  `public static final byte` | `RCP_TEST_QRY_REP` | `4`
  `public static final byte` | `RCP_TEST_QRYREP_REP` | `5`
  `public static final byte` | `RCP_TEST_SEL_REP` | `2`
  `public static final byte` | `RCP_UPDATE_FLASH` | `-46`