PhychipsRcp

com.ad.rfid.phychips

## 类 PhychipsRcp

- java.lang.Object
- - com.ad.rfid.ADRcp
  - - com.ad.rfid.phychips.PhychipsRcp

-     public class PhychipsRcp
      extends ADRcp

  Created by endyc on 2018-06-23.

- - ### 字段概要

    字段
    限定符和类型 | 字段和说明
    --- | ---
    `static byte` | `ENDMARK`
    `static byte` | `HEADER_CMD`
    `static byte` | `INDEX_ADDRESS` index address
    `static byte` | `INDEX_CODE` index code
    `static byte` | `INDEX_LENGTH` index length
    `static byte` | `INDEX_PAYLOAD` index payload
    `static byte` | `INDEX_PREAMBLE` index head
    `static byte` | `INDEX_TYPE` index type
    `static byte` | `LEN_CHECKSUM`
    `static byte` | `LEN_ENDMARK`
    `static byte` | `LEN_PROTOCOL_MIN` min len of protocol
    `static byte` | `PREAMBLE` send head
    `static byte` | `PREAMBLE_UP` receive head
    `static byte` | `RCP_CMD_AD_ADDR` Device Address
    `static byte` | `RCP_CMD_AD_CUSTOM` Base Paramters
    `static byte` | `RCP_CMD_AD_DATA` Limit Data Parameters
    `static byte` | `RCP_CMD_AD_IOOUT` IO Out Mode Paramters
    `static byte` | `RCP_CMD_AD_OUTCARD` Auto Out Data Paramters
    `static byte` | `RCP_CMD_AD_REMOTE` Remote IO
    `static byte` | `RCP_CMD_AD_UART` Change 232 and 485 Buadrate
    `static byte` | `RCP_CMD_BLOCKERASE_C_DT` BlockErase Type C User Data 0x48
    `static byte` | `RCP_CMD_BLOCKWRITE_C_DT` BlockWrite Type C User Data 0x47
    `static byte` | `RCP_CMD_CTL_RD_CON` Reader Connection Control
    `static byte` | `RCP_CMD_CTL_RD_PWR` Reader Power Control
    `static byte` | `RCP_CMD_CTL_RESET` Reset Reader
    `static byte` | `RCP_CMD_GET_ANTICOL_MODE`
    `static byte` | `RCP_CMD_GET_AT_RD_PARM` Get Automatic Read Parameters
    `static byte` | `RCP_CMD_GET_C_QRY_PARM` Get Type C A/I Query Related Parameters
    `static byte` | `RCP_CMD_GET_C_SEL_PARM` Get Type C A/I Select Parameters
    `static byte` | `RCP_CMD_GET_CH` Get Frequency Channel
    `static byte` | `RCP_CMD_GET_FH_LBT` Get Frequency Hopping
    `static byte` | `RCP_CMD_GET_HOPPING_TBL` Get Hopping table
    `static byte` | `RCP_CMD_GET_LAST_RST` Get Last Result
    `static byte` | `RCP_CMD_GET_MODEM_REG` Get Modem Register
    `static byte` | `RCP_CMD_GET_MODEM92_REG`
    `static byte` | `RCP_CMD_GET_MODULATION` Get Hopping table
    `static byte` | `RCP_CMD_GET_RD_INF` Get Reader Information
    `static byte` | `RCP_CMD_GET_REGION` Get Region
    `static byte` | `RCP_CMD_GET_RF_REG` Get RF Register
    `static byte` | `RCP_CMD_GET_RSSI` Get RSSI
    `static byte` | `RCP_CMD_GET_RX_GAIN` Get Rx Gain
    `static byte` | `RCP_CMD_GET_SIG_ST` Get Signal Strength
    `static byte` | `RCP_CMD_GET_TX_MODULE_PWR`
    `static byte` | `RCP_CMD_GET_TX_PWR`
    `static byte` | `RCP_CMD_INFO` Base Information
    `static byte` | `RCP_CMD_INVALID` RCP Command Type
    `static byte` | `RCP_CMD_KILL_RECOM_C` Kill Type C Tag
    `static byte` | `RCP_CMD_LOCK_C` Lock Type C Tag
    `static byte` | `RCP_CMD_MODEM_SINGLEREAD`
    `static byte` | `RCP_CMD_NACK`
    `static byte` | `RCP_CMD_NXP_CALIBRATE` NXP_CALIBRATE
    `static byte` | `RCP_CMD_NXP_CHANGE_EAS` NXP_CHANGE_EA
    `static byte` | `RCP_CMD_NXP_EAS_ALARM` NXP_EAS_ALARM
    `static byte` | `RCP_CMD_NXP_READPROTECT` NXP READPROTECT
    `static byte` | `RCP_CMD_NXP_RESET_READPROTECT` NXP_RESET_READPROTECT
    `static byte` | `RCP_CMD_PERMALOCK_C` Block Permalock
    `static byte` | `RCP_CMD_READ_C_DT` Read Type C Data 0x29
    `static byte` | `RCP_CMD_READ_C_ENTIRE` Read Entire Type C Tag 0x26
    `static byte` | `RCP_CMD_READ_C_UII` // Read Type C UII 0x22
    `static byte` | `RCP_CMD_READ_C_USR_DT` Read Type C User Data 0x24
    `static byte` | `RCP_CMD_SCAN_RSSI` Scan RSSI
    `static byte` | `RCP_CMD_SECRET` Secret tag Hex:0x30
    `static byte` | `RCP_CMD_SET_ANT_PATH`
    `static byte` | `RCP_CMD_SET_ANTICOL_MODE`
    `static byte` | `RCP_CMD_SET_AT_RD_PARM` Set Automatic Read Parameters
    `static byte` | `RCP_CMD_SET_C_QRY_PARM` Set Type C A/I Query Related Parameters
    `static byte` | `RCP_CMD_SET_C_SEL_PARM` Set Type C A/I Select Parameters
    `static byte` | `RCP_CMD_SET_CH` Set Frequency Channel
    `static byte` | `RCP_CMD_SET_CW`
    `static byte` | `RCP_CMD_SET_DELI`
    `static byte` | `RCP_CMD_SET_DOWNLOAD` Set Download Mode
    `static byte` | `RCP_CMD_SET_DUMP` Set Dump Mode
    `static byte` | `RCP_CMD_SET_FH_LBT` Set Frequency Hopping
    `static byte` | `RCP_CMD_SET_HOPPING_TBL` Set Hopping table
    `static byte` | `RCP_CMD_SET_INV_MODE` Set Inventory Mode
    `static byte` | `RCP_CMD_SET_LED`
    `static byte` | `RCP_CMD_SET_MOD_BLF`
    `static byte` | `RCP_CMD_SET_MOD_DEPTH`
    `static byte` | `RCP_CMD_SET_MODEM_REG` Set Modem Register
    `static byte` | `RCP_CMD_SET_MODEM92_REG`
    `static byte` | `RCP_CMD_SET_MODULATION` Set Hopping table
    `static byte` | `RCP_CMD_SET_MODULE_TABLE`
    `static byte` | `RCP_CMD_SET_REGION` Set Resion
    `static byte` | `RCP_CMD_SET_RF_REG` Set RF Register
    `static byte` | `RCP_CMD_SET_RX_GAIN` Set Rx Gain
    `static byte` | `RCP_CMD_SET_SIG_ST` Set Signal Strength
    `static byte` | `RCP_CMD_SET_TX_MODULE_PWR`
    `static byte` | `RCP_CMD_SET_TX_OFFSET`
    `static byte` | `RCP_CMD_SET_TX_PWR`
    `static byte` | `RCP_CMD_SET_TX_PWR_CL`
    `static byte` | `RCP_CMD_STOP_AUTO_READ` Stop Automatic Read 0x27
    `static byte` | `RCP_CMD_STOP_AUTO_READ_EX` Stop Automatic Read 0x37
    `static byte` | `RCP_CMD_STOP_RX_TEST` Stop Receive Test
    `static byte` | `RCP_CMD_STOP_TEST_MOD` Stop Test Mode
    `static byte` | `RCP_CMD_STRT_AUTO_READ` OutStart Automatic Read 0x27
    `static byte` | `RCP_CMD_STRT_AUTO_READ_EX` OutStart Automatic Read 0x36
    `static byte` | `RCP_CMD_STRT_RX_TEST` OutStart Receive Test
    `static byte` | `RCP_CMD_STRT_TEST_MOD` OutStart Test Mode
    `static byte` | `RCP_CMD_VENDOR_SPECIFIC_02` Set Table
    `static byte` | `RCP_CMD_VENDOR_SPECIFIC_03` Get Table
    `static byte` | `RCP_CMD_VENDOR_SPECIFIC_04` Set Inventory Mode
    `static byte` | `RCP_CMD_VENDOR_SPECIFIC_05` Set Inventory Mode
    `static byte` | `RCP_CMD_WIFI_AP` Wifi Model AP Parameters
    `static byte` | `RCP_CMD_WIFI_DOWNLOAD` Enable Wifi Model Parameters Download
    `static byte` | `RCP_CMD_WIFI_PUB` Wifi Model Public Parameters
    `static byte` | `RCP_CMD_WIFI_STA` Wifi Model Sta Parameters
    `static byte` | `RCP_CMD_WRIT_C_DT` Write Type C User Data 0x46
    `static byte` | `RCP_ERASE_FLASH`
    `static byte` | `RCP_GET_MSG_BUF_CNT`
    `static byte` | `RCP_GET_REGISTRY_ITEM`
    `static byte` | `RCP_GET_TEMPERATURE` Get Chip Temperature
    `static byte` | `RCP_MSG_AUTO` Auto Send
    `static byte` | `RCP_MSG_CAP`
    `static byte` | `RCP_MSG_CMD` Command Type
    `static byte` | `RCP_MSG_GET` Get Type
    `static byte` | `RCP_MSG_NOTI` Notification Type
    `static byte` | `RCP_MSG_RSP` Response Type
    `static byte` | `RCP_MSG_SET` Set Type
    `static byte` | `RCP_MSG_TEST` Test Type
    `static byte` | `RCP_SET_INT_PARAM`
    `static byte` | `RCP_SET_LT`
    `static byte` | `RCP_SET_REGISTRY_ITEM`
    `static byte` | `RCP_TEST_EPC_QRYACK`
    `static byte` | `RCP_TEST_EPC_QRYQRYREP`
    `static byte` | `RCP_TEST_EPC_SEL`
    `static byte` | `RCP_TEST_EPC_SELQRY`
    `static byte` | `RCP_TEST_MODEM_RX` Test Modem Rx
    `static byte` | `RCP_TEST_MODEM_SEL_REP_E` Test Modem Select Repeat End
    `static byte` | `RCP_TEST_PKT_CAP_ACK`
    `static byte` | `RCP_TEST_PKT_CAP_UII`
    `static byte` | `RCP_TEST_PKT_CAPTURE`
    `static byte` | `RCP_TEST_QRY_REP` Test Select Query Repeat
    `static byte` | `RCP_TEST_QRYREP_REP` Test Select QueryReq Repeat
    `static byte` | `RCP_TEST_SEL_REP` Test Modem Select Repeat OutStart
    `static byte` | `RCP_UPDATE_FLASH`

  - ### 构造器概要

    构造器
    构造器和说明
    `PhychipsRcp()`
    `PhychipsRcp(ADSio sio)`

  - ### 方法概要

    所有方法 实例方法 具体方法
    限定符和类型 | 方法和说明
    --- | ---
    `byte[]` | `buildCmdPacketByte(byte nType, byte nCmd, byte[] ArgByte)` packet command data (打包命令数据)
    `byte[]` | `buildCmdPacketByte(int nAddr, byte nType, byte nCmd, byte[] ArgByte)` packet command data (打包命令数据)
    `void` | `dealPacketByte(ByteEventArg e)`

    - ### 从类继承的方法 com.ad.rfid.ADRcp

      `addOnProtocolListener, buildCmdPacketByte, connect, disConnect, getAddress, getDelay, getDeviceMode, getMode, getRcpReceivedPacket, getType, getVersion, isConnected, removeOnProtocolListener, sendBytePkt, sendBytePkt, setAddress, setDelay, setMode, setOnProtocolListener, setSio, setType, setVersion`

    - ### 从类继承的方法 java.lang.Object

      `equals, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

- - ### 字段详细资料

    - #### PREAMBLE

          public static final byte PREAMBLE

      send head
      另请参阅:
        常量字段值

    - #### PREAMBLE_UP

          public static final byte PREAMBLE_UP

      receive head
      另请参阅:
        常量字段值

    - #### INDEX_PREAMBLE

          public static final byte INDEX_PREAMBLE

      index head
      另请参阅:
        常量字段值

    - #### INDEX_ADDRESS

          public static final byte INDEX_ADDRESS

      index address
      另请参阅:
        常量字段值

    - #### INDEX_CODE

          public static final byte INDEX_CODE

      index code
      另请参阅:
        常量字段值

    - #### INDEX_TYPE

          public static final byte INDEX_TYPE

      index type
      另请参阅:
        常量字段值

    - #### INDEX_LENGTH

          public static final byte INDEX_LENGTH

      index length
      另请参阅:
        常量字段值

    - #### INDEX_PAYLOAD

          public static final byte INDEX_PAYLOAD

      index payload
      另请参阅:
        常量字段值

    - #### LEN_ENDMARK

          public static final byte LEN_ENDMARK

      另请参阅:
        常量字段值

    - #### LEN_CHECKSUM

          public static final byte LEN_CHECKSUM

      另请参阅:
        常量字段值

    - #### LEN_PROTOCOL_MIN

          public static final byte LEN_PROTOCOL_MIN

      min len of protocol
      另请参阅:
        常量字段值

    - #### ENDMARK

          public static final byte ENDMARK

      另请参阅:
        常量字段值

    - #### HEADER_CMD

          public static final byte HEADER_CMD

      另请参阅:
        常量字段值

    - #### RCP_MSG_CMD

          public static final byte RCP_MSG_CMD

      Command Type
      另请参阅:
        常量字段值

    - #### RCP_MSG_RSP

          public static final byte RCP_MSG_RSP

      Response Type
      另请参阅:
        常量字段值

    - #### RCP_MSG_NOTI

          public static final byte RCP_MSG_NOTI

      Notification Type
      另请参阅:
        常量字段值

    - #### RCP_MSG_TEST

          public static final byte RCP_MSG_TEST

      Test Type
      另请参阅:
        常量字段值

    - #### RCP_MSG_CAP

          public static final byte RCP_MSG_CAP

      另请参阅:
        常量字段值

    - #### RCP_MSG_AUTO

          public static final byte RCP_MSG_AUTO

      Auto Send
      另请参阅:
        常量字段值

    - #### RCP_MSG_SET

          public static final byte RCP_MSG_SET

      Set Type
      另请参阅:
        常量字段值

    - #### RCP_MSG_GET

          public static final byte RCP_MSG_GET

      Get Type
      另请参阅:
        常量字段值

    - #### RCP_CMD_INVALID

          public static final byte RCP_CMD_INVALID

      RCP Command Type
      另请参阅:
        常量字段值

    - #### RCP_CMD_CTL_RD_PWR

          public static final byte RCP_CMD_CTL_RD_PWR

      Reader Power Control
      另请参阅:
        常量字段值

    - #### RCP_CMD_CTL_RD_CON

          public static final byte RCP_CMD_CTL_RD_CON

      Reader Connection Control
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_RD_INF

          public static final byte RCP_CMD_GET_RD_INF

      Get Reader Information
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_SIG_ST

          public static final byte RCP_CMD_GET_SIG_ST

      Get Signal Strength
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_SIG_ST

          public static final byte RCP_CMD_SET_SIG_ST

      Set Signal Strength
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_REGION

          public static final byte RCP_CMD_GET_REGION

      Get Region
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_REGION

          public static final byte RCP_CMD_SET_REGION

      Set Resion
      另请参阅:
        常量字段值

    - #### RCP_CMD_CTL_RESET

          public static final byte RCP_CMD_CTL_RESET

      Reset Reader
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_CH

          public static final byte RCP_CMD_GET_CH

      Get Frequency Channel
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_CH

          public static final byte RCP_CMD_SET_CH

      Set Frequency Channel
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_FH_LBT

          public static final byte RCP_CMD_GET_FH_LBT

      Get Frequency Hopping
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_FH_LBT

          public static final byte RCP_CMD_SET_FH_LBT

      Set Frequency Hopping
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_TX_PWR

          public static final byte RCP_CMD_GET_TX_PWR

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_TX_PWR

          public static final byte RCP_CMD_SET_TX_PWR

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_CW

          public static final byte RCP_CMD_SET_CW

      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_C_SEL_PARM

          public static final byte RCP_CMD_GET_C_SEL_PARM

      Get Type C A/I Select Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_C_SEL_PARM

          public static final byte RCP_CMD_SET_C_SEL_PARM

      Set Type C A/I Select Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_C_QRY_PARM

          public static final byte RCP_CMD_GET_C_QRY_PARM

      Get Type C A/I Query Related Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_C_QRY_PARM

          public static final byte RCP_CMD_SET_C_QRY_PARM

      Set Type C A/I Query Related Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_AT_RD_PARM

          public static final byte RCP_CMD_GET_AT_RD_PARM

      Get Automatic Read Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_AT_RD_PARM

          public static final byte RCP_CMD_SET_AT_RD_PARM

      Set Automatic Read Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_INV_MODE

          public static final byte RCP_CMD_SET_INV_MODE

      Set Inventory Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_VENDOR_SPECIFIC_02

          public static final byte RCP_CMD_VENDOR_SPECIFIC_02

      Set Table
      另请参阅:
        常量字段值

    - #### RCP_CMD_VENDOR_SPECIFIC_03

          public static final byte RCP_CMD_VENDOR_SPECIFIC_03

      Get Table
      另请参阅:
        常量字段值

    - #### RCP_CMD_VENDOR_SPECIFIC_04

          public static final byte RCP_CMD_VENDOR_SPECIFIC_04

      Set Inventory Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_VENDOR_SPECIFIC_05

          public static final byte RCP_CMD_VENDOR_SPECIFIC_05

      Set Inventory Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_READ_C_UII

          public static final byte RCP_CMD_READ_C_UII

      // Read Type C UII 0x22
      另请参阅:
        常量字段值

    - #### RCP_CMD_READ_C_USR_DT

          public static final byte RCP_CMD_READ_C_USR_DT

      Read Type C User Data 0x24
      另请参阅:
        常量字段值

    - #### RCP_CMD_READ_C_ENTIRE

          public static final byte RCP_CMD_READ_C_ENTIRE

      Read Entire Type C Tag 0x26
      另请参阅:
        常量字段值

    - #### RCP_CMD_STRT_AUTO_READ

          public static final byte RCP_CMD_STRT_AUTO_READ

      OutStart Automatic Read 0x27
      另请参阅:
        常量字段值

    - #### RCP_CMD_STOP_AUTO_READ

          public static final byte RCP_CMD_STOP_AUTO_READ

      Stop Automatic Read 0x27
      另请参阅:
        常量字段值

    - #### RCP_CMD_READ_C_DT

          public static final byte RCP_CMD_READ_C_DT

      Read Type C Data 0x29
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_HOPPING_TBL

          public static final byte RCP_CMD_GET_HOPPING_TBL

      Get Hopping table
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_HOPPING_TBL

          public static final byte RCP_CMD_SET_HOPPING_TBL

      Set Hopping table
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_MODULATION

          public static final byte RCP_CMD_GET_MODULATION

      Get Hopping table
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_MODULATION

          public static final byte RCP_CMD_SET_MODULATION

      Set Hopping table
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_ANTICOL_MODE

          public static final byte RCP_CMD_GET_ANTICOL_MODE

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_ANTICOL_MODE

          public static final byte RCP_CMD_SET_ANTICOL_MODE

      另请参阅:
        常量字段值

    - #### RCP_CMD_STRT_AUTO_READ_EX

          public static final byte RCP_CMD_STRT_AUTO_READ_EX

      OutStart Automatic Read 0x36
      另请参阅:
        常量字段值

    - #### RCP_CMD_STOP_AUTO_READ_EX

          public static final byte RCP_CMD_STOP_AUTO_READ_EX

      Stop Automatic Read 0x37
      另请参阅:
        常量字段值

    - #### RCP_CMD_WRIT_C_DT

          public static final byte RCP_CMD_WRIT_C_DT

      Write Type C User Data 0x46
      另请参阅:
        常量字段值

    - #### RCP_CMD_BLOCKWRITE_C_DT

          public static final byte RCP_CMD_BLOCKWRITE_C_DT

      BlockWrite Type C User Data 0x47
      另请参阅:
        常量字段值

    - #### RCP_CMD_BLOCKERASE_C_DT

          public static final byte RCP_CMD_BLOCKERASE_C_DT

      BlockErase Type C User Data 0x48
      另请参阅:
        常量字段值

    - #### RCP_CMD_NXP_READPROTECT

          public static final byte RCP_CMD_NXP_READPROTECT

      NXP READPROTECT
      另请参阅:
        常量字段值

    - #### RCP_CMD_NXP_RESET_READPROTECT

          public static final byte RCP_CMD_NXP_RESET_READPROTECT

      NXP_RESET_READPROTECT
      另请参阅:
        常量字段值

    - #### RCP_CMD_NXP_CHANGE_EAS

          public static final byte RCP_CMD_NXP_CHANGE_EAS

      NXP_CHANGE_EA
      另请参阅:
        常量字段值

    - #### RCP_CMD_NXP_EAS_ALARM

          public static final byte RCP_CMD_NXP_EAS_ALARM

      NXP_EAS_ALARM
      另请参阅:
        常量字段值

    - #### RCP_CMD_NXP_CALIBRATE

          public static final byte RCP_CMD_NXP_CALIBRATE

      NXP_CALIBRATE
      另请参阅:
        常量字段值

    - #### RCP_CMD_KILL_RECOM_C

          public static final byte RCP_CMD_KILL_RECOM_C

      Kill Type C Tag
      另请参阅:
        常量字段值

    - #### RCP_CMD_LOCK_C

          public static final byte RCP_CMD_LOCK_C

      Lock Type C Tag
      另请参阅:
        常量字段值

    - #### RCP_CMD_PERMALOCK_C

          public static final byte RCP_CMD_PERMALOCK_C

      Block Permalock
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_DOWNLOAD

          public static final byte RCP_CMD_SET_DOWNLOAD

      Set Download Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_DUMP

          public static final byte RCP_CMD_SET_DUMP

      Set Dump Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_MODEM92_REG

          public static final byte RCP_CMD_SET_MODEM92_REG

      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_MODEM92_REG

          public static final byte RCP_CMD_GET_MODEM92_REG

      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_LAST_RST

          public static final byte RCP_CMD_GET_LAST_RST

      Get Last Result
      另请参阅:
        常量字段值

    - #### RCP_CMD_STRT_TEST_MOD

          public static final byte RCP_CMD_STRT_TEST_MOD

      OutStart Test Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_STOP_TEST_MOD

          public static final byte RCP_CMD_STOP_TEST_MOD

      Stop Test Mode
      另请参阅:
        常量字段值

    - #### RCP_CMD_STRT_RX_TEST

          public static final byte RCP_CMD_STRT_RX_TEST

      OutStart Receive Test
      另请参阅:
        常量字段值

    - #### RCP_CMD_STOP_RX_TEST

          public static final byte RCP_CMD_STOP_RX_TEST

      Stop Receive Test
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_MODEM_REG

          public static final byte RCP_CMD_SET_MODEM_REG

      Set Modem Register
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_RF_REG

          public static final byte RCP_CMD_SET_RF_REG

      Set RF Register
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_MODEM_REG

          public static final byte RCP_CMD_GET_MODEM_REG

      Get Modem Register
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_RF_REG

          public static final byte RCP_CMD_GET_RF_REG

      Get RF Register
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_TX_MODULE_PWR

          public static final byte RCP_CMD_SET_TX_MODULE_PWR

      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_TX_MODULE_PWR

          public static final byte RCP_CMD_GET_TX_MODULE_PWR

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_ANT_PATH

          public static final byte RCP_CMD_SET_ANT_PATH

      另请参阅:
        常量字段值

    - #### RCP_GET_TEMPERATURE

          public static final byte RCP_GET_TEMPERATURE

      Get Chip Temperature
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_TX_OFFSET

          public static final byte RCP_CMD_SET_TX_OFFSET

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_TX_PWR_CL

          public static final byte RCP_CMD_SET_TX_PWR_CL

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_MOD_DEPTH

          public static final byte RCP_CMD_SET_MOD_DEPTH

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_MODULE_TABLE

          public static final byte RCP_CMD_SET_MODULE_TABLE

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_DELI

          public static final byte RCP_CMD_SET_DELI

      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_MOD_BLF

          public static final byte RCP_CMD_SET_MOD_BLF

      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_RX_GAIN

          public static final byte RCP_CMD_GET_RX_GAIN

      Get Rx Gain
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_RX_GAIN

          public static final byte RCP_CMD_SET_RX_GAIN

      Set Rx Gain
      另请参阅:
        常量字段值

    - #### RCP_CMD_GET_RSSI

          public static final byte RCP_CMD_GET_RSSI

      Get RSSI
      另请参阅:
        常量字段值

    - #### RCP_CMD_SCAN_RSSI

          public static final byte RCP_CMD_SCAN_RSSI

      Scan RSSI
      另请参阅:
        常量字段值

    - #### RCP_SET_INT_PARAM

          public static final byte RCP_SET_INT_PARAM

      另请参阅:
        常量字段值

    - #### RCP_UPDATE_FLASH

          public static final byte RCP_UPDATE_FLASH

      另请参阅:
        常量字段值

    - #### RCP_ERASE_FLASH

          public static final byte RCP_ERASE_FLASH

      另请参阅:
        常量字段值

    - #### RCP_GET_REGISTRY_ITEM

          public static final byte RCP_GET_REGISTRY_ITEM

      另请参阅:
        常量字段值

    - #### RCP_SET_REGISTRY_ITEM

          public static final byte RCP_SET_REGISTRY_ITEM

      另请参阅:
        常量字段值

    - #### RCP_GET_MSG_BUF_CNT

          public static final byte RCP_GET_MSG_BUF_CNT

      另请参阅:
        常量字段值

    - #### RCP_SET_LT

          public static final byte RCP_SET_LT

      另请参阅:
        常量字段值

    - #### RCP_CMD_MODEM_SINGLEREAD

          public static final byte RCP_CMD_MODEM_SINGLEREAD

      另请参阅:
        常量字段值

    - #### RCP_CMD_NACK

          public static final byte RCP_CMD_NACK

      另请参阅:
        常量字段值

    - #### RCP_TEST_MODEM_RX

          public static final byte RCP_TEST_MODEM_RX

      Test Modem Rx
      另请参阅:
        常量字段值

    - #### RCP_TEST_SEL_REP

          public static final byte RCP_TEST_SEL_REP

      Test Modem Select Repeat OutStart
      另请参阅:
        常量字段值

    - #### RCP_TEST_MODEM_SEL_REP_E

          public static final byte RCP_TEST_MODEM_SEL_REP_E

      Test Modem Select Repeat End
      另请参阅:
        常量字段值

    - #### RCP_TEST_QRY_REP

          public static final byte RCP_TEST_QRY_REP

      Test Select Query Repeat
      另请参阅:
        常量字段值

    - #### RCP_TEST_QRYREP_REP

          public static final byte RCP_TEST_QRYREP_REP

      Test Select QueryReq Repeat
      另请参阅:
        常量字段值

    - #### RCP_TEST_EPC_SEL

          public static final byte RCP_TEST_EPC_SEL

      另请参阅:
        常量字段值

    - #### RCP_TEST_EPC_SELQRY

          public static final byte RCP_TEST_EPC_SELQRY

      另请参阅:
        常量字段值

    - #### RCP_TEST_EPC_QRYACK

          public static final byte RCP_TEST_EPC_QRYACK

      另请参阅:
        常量字段值

    - #### RCP_TEST_EPC_QRYQRYREP

          public static final byte RCP_TEST_EPC_QRYQRYREP

      另请参阅:
        常量字段值

    - #### RCP_TEST_PKT_CAPTURE

          public static final byte RCP_TEST_PKT_CAPTURE

      另请参阅:
        常量字段值

    - #### RCP_TEST_PKT_CAP_ACK

          public static final byte RCP_TEST_PKT_CAP_ACK

      另请参阅:
        常量字段值

    - #### RCP_TEST_PKT_CAP_UII

          public static final byte RCP_TEST_PKT_CAP_UII

      另请参阅:
        常量字段值

    - #### RCP_CMD_SECRET

          public static final byte RCP_CMD_SECRET

      Secret tag Hex:0x30
      另请参阅:
        常量字段值

    - #### RCP_CMD_INFO

          public static final byte RCP_CMD_INFO

      Base Information
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_REMOTE

          public static final byte RCP_CMD_AD_REMOTE

      Remote IO
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_CUSTOM

          public static final byte RCP_CMD_AD_CUSTOM

      Base Paramters
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_ADDR

          public static final byte RCP_CMD_AD_ADDR

      Device Address
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_OUTCARD

          public static final byte RCP_CMD_AD_OUTCARD

      Auto Out Data Paramters
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_IOOUT

          public static final byte RCP_CMD_AD_IOOUT

      IO Out Mode Paramters
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_DATA

          public static final byte RCP_CMD_AD_DATA

      Limit Data Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_AD_UART

          public static final byte RCP_CMD_AD_UART

      Change 232 and 485 Buadrate
      另请参阅:
        常量字段值

    - #### RCP_CMD_WIFI_DOWNLOAD

          public static final byte RCP_CMD_WIFI_DOWNLOAD

      Enable Wifi Model Parameters Download
      另请参阅:
        常量字段值

    - #### RCP_CMD_WIFI_PUB

          public static final byte RCP_CMD_WIFI_PUB

      Wifi Model Public Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_WIFI_STA

          public static final byte RCP_CMD_WIFI_STA

      Wifi Model Sta Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_WIFI_AP

          public static final byte RCP_CMD_WIFI_AP

      Wifi Model AP Parameters
      另请参阅:
        常量字段值

    - #### RCP_CMD_SET_LED

          public static final byte RCP_CMD_SET_LED

      另请参阅:
        常量字段值

  - ### 构造器详细资料

    - #### PhychipsRcp

          public PhychipsRcp()

    - #### PhychipsRcp

          public PhychipsRcp(ADSio sio)

  - ### 方法详细资料

    - #### buildCmdPacketByte

          public byte[] buildCmdPacketByte(byte nType,
                                           byte nCmd,
                                           byte[] ArgByte)

      从类复制的说明: `ADRcp`
      packet command data (打包命令数据)
      指定者:
        `buildCmdPacketByte` 在类中 `ADRcp`
      参数:
        `nType` - 命令方式,get of set
        `nCmd` - 命令类型
        `ArgByte` - 数据
      返回:

    - #### buildCmdPacketByte

          public byte[] buildCmdPacketByte(int nAddr,
                                           byte nType,
                                           byte nCmd,
                                           byte[] ArgByte)

      从类复制的说明: `ADRcp`
      packet command data (打包命令数据)
      指定者:
        `buildCmdPacketByte` 在类中 `ADRcp`
      参数:
        `nAddr` - 通讯地址
        `nType` - 命令方式,get of set
        `nCmd` - 命令类型
        `ArgByte` - 数据
      返回:

    - #### dealPacketByte

          public void dealPacketByte(ByteEventArg e)