U - 索引

A B C D E F G H I K L M N O P R S T U W X

## U

UpdateRegistry(ADRcp) - 类 中的静态方法com.ad.rfid.phychips.PhychipsCommand
  Registry Update
USB - 类 中的静态变量com.ad.comm.CommType
USB_CLASS_APP_SPEC - 类 中的静态变量com.ad.comm.usb.ADConstants
  Application specific USB class.
USB_CLASS_AUDIO - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for audio devices.
USB_CLASS_CDC_DATA - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for CDC devices (communications device class).
USB_CLASS_COMM - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for communication devices.
USB_CLASS_CONTENT_SEC - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for content security devices.
USB_CLASS_CSCID - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for content smart card devices.
USB_CLASS_HID - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for human interface devices (for example, mice and keyboards).
USB_CLASS_HUB - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for USB hubs.
USB_CLASS_MASS_STORAGE - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for mass storage devices.
USB_CLASS_MISC - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for wireless miscellaneous devices.
USB_CLASS_PER_INTERFACE - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class indicating that the class is determined on a per-interface basis.
USB_CLASS_PHYSICA - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for physical devices.
USB_CLASS_PRINTER - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for printers.
USB_CLASS_STILL_IMAGE - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for still image devices (digital cameras).
USB_CLASS_VENDOR_SPEC - 类 中的静态变量com.ad.comm.usb.ADConstants
  Vendor specific USB class.
USB_CLASS_VIDEO - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for video devices.
USB_CLASS_WIRELESS_CONTROLLER - 类 中的静态变量com.ad.comm.usb.ADConstants
  USB class for wireless controller devices.
USB_DIR_IN - 类 中的静态变量com.ad.comm.usb.ADConstants
  Used to signify direction of data for a `UsbEndpoint` is IN (device to host)
USB_DIR_OUT - 类 中的静态变量com.ad.comm.usb.ADConstants
  Used to signify direction of data for a `UsbEndpoint` is OUT (host to device)
USB_ENDPOINT_DIR_MASK - 类 中的静态变量com.ad.comm.usb.ADConstants
  Bitmask used for extracting the `UsbEndpoint` direction from its address field.
USB_ENDPOINT_NUMBER_MASK - 类 中的静态变量com.ad.comm.usb.ADConstants
  Bitmask used for extracting the `UsbEndpoint` number its address field.
USB_ENDPOINT_XFER_BULK - 类 中的静态变量com.ad.comm.usb.ADConstants
  Bulk endpoint type
USB_ENDPOINT_XFER_CONTROL - 类 中的静态变量com.ad.comm.usb.ADConstants
  Control endpoint type (endpoint zero)
USB_ENDPOINT_XFER_INT - 类 中的静态变量com.ad.comm.usb.ADConstants
  Interrupt endpoint type
USB_ENDPOINT_XFER_ISOC - 类 中的静态变量com.ad.comm.usb.ADConstants
  Isochronous endpoint type (currently not supported)
USB_ENDPOINT_XFERTYPE_MASK - 类 中的静态变量com.ad.comm.usb.ADConstants
  Bitmask used for extracting the `UsbEndpoint` type from its address field.
USB_INTERFACE_SUBCLASS_BOOT - 类 中的静态变量com.ad.comm.usb.ADConstants
  Boot subclass for HID devices.
USB_SUBCLASS_VENDOR_SPEC - 类 中的静态变量com.ad.comm.usb.ADConstants
  Vendor specific USB subclass.
USB_TYPE_CLASS - 类 中的静态变量com.ad.comm.usb.ADConstants
  Used to specify that an endpoint zero control request is a class specific request.
USB_TYPE_MASK - 类 中的静态变量com.ad.comm.usb.ADConstants
  Bitmask used for encoding the request type for a control request on endpoint zero.
USB_TYPE_RESERVED - 类 中的静态变量com.ad.comm.usb.ADConstants
  Reserved endpoint zero control request type (currently unused).
USB_TYPE_STANDARD - 类 中的静态变量com.ad.comm.usb.ADConstants
  Used to specify that an endpoint zero control request is a standard request.
USB_TYPE_VENDOR - 类 中的静态变量com.ad.comm.usb.ADConstants
  Used to specify that an endpoint zero control request is a vendor specific request.

A B C D E F G H I K L M N O P R S T U W X